bootargs=console=ttyPS0,115200 root=/dev/mmcblk0p2 rootwait rw earlyprintk
ethaddr=00:0a:35:00:01:21
kernel_load_address=0x3000000
kernel_image=uImage
devicetree_load_address=0x2A00000
devicetree_image=devicetree.dtb
sdboot=if mmcinfo; then load mmc 0 ${kernel_load_address} ${kernel_image} && load mmc 0 ${devicetree_load_address} ${devicetree_image} && bootm ${kernel_load_address} - ${devicetree_load_address}; fi
autoload=y
